

**MIDDLE EAST TECHNICAL UNIVERSITY**

**DEPARTMENT OF ELECTRICAL & ELECTRONICS ENGINEERING**

**EE 464 - Static Power Conversion II - Term Project**

**Social Isolation Inc.**

**Development of a DC-DC Converter for Battery Charging**

**Berkay Uzun - 2263812**

**Ali BELLİ - 2231421**

**Ahmet Halis Sabırlı – 2305225**

Table of Contents

[1.Project Definition 3](#_Toc70621159)

[2. Topology Selection 3](#_Toc70621160)

[3. Controller Selection 4](#_Toc70621161)

[4. Transformer Design 6](#_Toc70621162)

[4.1. Magnetic Core Selection 6](#_Toc70621163)

[4.2. Winding Selection 11](#_Toc70621164)

[4.3. Finite Element Analysis 11](#_Toc70621165)

[5. Component Selection 15](#_Toc70621166)

[5.1 Output Capacitor Selection 15](#_Toc70621167)

[5.2 Controller Passive Elements Selection 16](#_Toc70621168)

[5.2.1 Snubber Resistance Selection 16](#_Toc70621169)

[5.2.2 Feedback Resistances Selection 16](#_Toc70621170)

[5.2.3 RIREG/SS Selection 17](#_Toc70621171)

[5.2.4 Sense Resistor Selection 17](#_Toc70621172)

[5.2.5 Boundary Mode Detection Capacitor 18](#_Toc70621173)

[5.2.6 Additional Component 18](#_Toc70621174)

[5.3 Semiconductor Selection 18](#_Toc70621175)

[5.3.1 Snubber Diodes Selection 18](#_Toc70621176)

[5.3.2 MOSFET Selection 19](#_Toc70621177)

[5.3.3 Output Diode Selection 20](#_Toc70621178)

[6. LTspice Simulation Results 21](#_Toc70621179)

[6.1 Steady-State Full-Load Responses 22](#_Toc70621180)

[6.2 Load Regulation 23](#_Toc70621181)

[6.3 Line Regulation 24](#_Toc70621182)

[7. Conclusion 25](#_Toc70621183)

[8. References 25](#_Toc70621184)

# 1.Project Definition

In electrical cars, inside the vehicle, there are two different electrical systems which are low voltage and high voltage. The use of low voltage is to run the low power and low voltage components of the vehicle such as monitor, audio player or fans of the cooling system. To be able to charge the low voltage battery, there is a need of DC/DC converter between high voltage and low voltage system. The main motivation of the project is to construct an isolated 100W DC/DC converter which steps down the 220-400 V input to the 12 V output.

# 2. Topology Selection

For the topology selection, there is only one main consideration which is the output power level. The selected topology must satisfy the output power and should not be over designed on it. To do that, we have made some research and found the source to decide the topology. From the information given in Table 1, there are 5 options [1].

Table 1- Power ranges of some of isolated DC-DC converter topologies

|  |  |
| --- | --- |
| **TOPOLOGY** | **POWER RANGE HISTORICALLY USED** |
| **Flyback** | <100 W |
| **Forward** | 50W-200W |
| **Active Clamp Forward** | 50W-300W |
| **Push-Pull** | 100W-500W |
| **Half-Bridge** | 100W-500W |
| **Full-Bridge** | >500W |

When we look at the options, the Full-Bridge is not suitable. In addition, we can see that Push-Pull and Half-Bridge may be over design for our application because the lower limit of them is satisfying the maximum power requirement of our system. Therefore, they are not suitable for our application. After that point, there are staying 3 different topologies. Forward and Active Clamp Forward has more component compared to the Flyback converter and the Flyback converters maximum power limitation is satisfying our power level. Because of these reasons, we decided to use the Flyback topology to design the DC-DC converter. In addition to them, Flyback is a widely used topology and there are a lot of sources and controllers for this topology in power electronics field. Therefore, easy implementation of the topology has also made us to choose this topology.




Figure 1. Flyback converter topology.

# 3. Controller Selection

For the controller selection, we have only found two different controllers of the Analog Devices for our application. One of them is Forward and the other one is Flyback converter. The main limitation on the controllers is the maximum input voltage. Although, we have checked so many different producers’ controllers, we did not find suitable controllers other than the LT8316 and LT3752-1. The main typical applications of the controllers are given in Fig.-1 and Fig.-2.



Figure 2. LT3752-1 Typical use.

Figure 3. LT8316 Typical use.

As the consideration given in the topology selection session, the Forward controller requires more component than the Flyback controller. Therefore, we have chosen the LT8316 DC-DC Flyback controller to develop the converter.

# 4. Transformer Design

In this part of the project, the following steps were done, the Magnetic Core Design, Winding Selection and Finite Element analysis. To do that, at first, we examined the Flyback topology and developed and Excel program to find the proper interval of inductance and turning ratios. There are mainly to considerations to find the intervals, which are the properties of the controller and the requirements of the Flyback topology. Before going into the calculations of the controller, we calculated the topology requirements for these conditions. After that we obtained the controller needs and intervals. By considering the results, we decided on which core we will use. When we finished the core selection, we began to clarify the wiring properties which are depended on the effective window area of the core and current flowing through wirings. After completing the wire and core selection parts, we run a finite element on ANYSY to check whether our transformer going into the saturation or not. By proving the non-saturated behavior of the core during the maximum limits of the operation, we finished the Transformer Design part.

## 4.1. Magnetic Core Selection

Before going through the design, at first, we need to decide how we make design, in other words we need to fix some of the parameters to find the rest of the values. We decided to fix the desired duty cycle, desired current ripple, estimated efficiency, and the switching frequency. The switching frequency and the desired current ripple are fixed by considering the operation of the converter. After the fixing the values, the theoretical calculation of the Flyback topology going through like that,

We need to find some important variables of the circuit to continue the calculations,

The ratio is hard to find a proper turn numbers of the primary and secondary, therefore,

After deciding the turn, we need calculate estimated duty cycle of the system to find the turn number of the primary and secondary windings.

Now, let’s find the maximum turn number of the primary side,

As you can observe, we need the find a core to use the effective core area (Ac) and the saturation flux density (Bsat). Selecting the core is not straight forward issue. We selected it by checking the limitations again and again for different cores. The limitations will be calculated later. We selected one of the cores of TDK, which is ETD 29/16/10. The selected core properties are given in the Table 2.

Table 2- Selected magnetic Mn-Zn ETD shape core

|  |  |
| --- | --- |
| **PROPERTIES** | **VALUES** |
| **Saturation Flux Density(T)** | 0.39 |
| **Effective magnetic cross section(mm2)** | 76 |
| **Window Area (Winding Cross Section) (mm2)** | 97 |
| **Inductance Factor(nH/turn2)** | 383 |
| **Average Length of Turn(mm)** | 52.8 |
| **Effective magnetic path length (mm)** | 70.4 |
| **Relative permeability of core material (Ungapped)** | 1470 |
| **Relative permeability of core material (Gapped)** | 281 |
| **Airgap(mm)** | 0.2 |

We decided to use the primary turn as 25 and secondary as 3. Now, we need to calculate the final, effective, duty cycle,

Now, let’s find the effective inductance values for %100 inductor current ripple,

After finishing the theoretical calculations, now we need the find the limitations of the controller. There are 3 different minimum primary inductance limitation and one maximum primary inductance limitation. Before starting to the calculations, there are some parameters must be given which are used in the following calculations coming from the nature of the controller.

By using the core properties, we can calculate the primary and secondary inductances and check whether we stay in the controller specifications or not and whether we close to theoretical calculations.

The selection of the inductance factor (AL) is not a straightforward issue and we selected it by considering the saturation limit of the selected core. Therefore, we have had to lose some inductance to satisfy the non-saturated operation and to leave the final duty cycle lower than the desired one. As a result, the inductance values are suitable for the controller and the controller will handle rest of the parameters by using the feedback loop inside it.

We checked how much airgap we need to stay in the non-saturated region during the operation,

We have used the equation given below to check whether the core is going through the saturation during the operation or not,

We are satisfying saturation condition, which is the most important one for the application. At that point, we are finishing the core selection part and moving to the winding selection part.

## 4.2. Winding Selection

Winding selection is another important topic while designing a transformer. Both the wire itself and the wiring type effects the performance of the transformer. Choosing thicker wire may seem to reduce the resistance and losses however due to skin and proximity effects, diameter of the wire does not affect losses after a point. Moreover, thicker wires results in bulkier windings which increases leakage inductances. However, choosing wires too thin may result in excessive heat generation and meltdown in critical points of the winding. Therefore, we tried to make a balanced selection.

First, we assumed that output current flows through the windings without alternating and find a wire so that current density of the wire is around 5 A/mm2

Even though, due to skin and proximity effects, current will flow nonhomogeneous and most of the copper will not carry any current, high heat capacitance of thicker wire will prevent burnouts in the winding.

We have total of 31 turns of winding which consists of 25 primary, 3 secondary and 3 feedback turns. The selected core can accommodate around 12-13 turns per layer. Since we only needed three layers of windings, we did not see necessary to make interleaved winding and make two layers of primary winding and one layer of combined secondary and feedback winding.

## 4.3. Finite Element Analysis

After deciding the core material, shape, airgap and the windings, we started to draw the transformer in Maxwell 3D. For faster analysis, continuous surfaces were drawn with edges as shown in Fig 5. Main reason of Finite Element Analysis is to check our design parameters and calculate transformer parameters which cannot be calculated analytically. First, we draw only the primary winding to check our model’s validity. After finding that analysis results were almost same with datasheet values of the core we continued with secondary and feedback windings. However, if we make 25 turn primary and 3 turn secondary, secondary inductance becomes larger than the calculations. This is most probably due to reduction of magnetic path (therefore reduction in reluctance) while increasing layer number (winding radius). This kind of secondary effects was the first reason why we did finite element analysis. To overcome this effect, we reduced the secondary turn number to 2.5 and the results were satisfactory.




Figure 4. Self and mutual inductances of the windings (μH).





Figure 5. Maxwell 3D model.

After satisfying inductance and turn ratio parameters we moved on to saturation control. To observe the magnetic flux density in most extreme case, we supplied primary winding with 3A current. This 3A comes from the calculations of the controller and it is also observed in LTspice. To ease the work of the computer, meshing was concentrated in the inner corner and near the airgap. Both magnetic flux density and vectors can be seen in Fig 6,7 and 8.




Figure 6. Magnetic flux vectors.




Figure 7. Magnetic flux density.




Figure 8. Magnetic flux density of the core center.

At maximum magnetic flux density that the core can see, most of the core remans unsaturated. However, some corners of the core are saturated. This may be acceptable since transformer will work in this condition on extreme cases and for transient times. Transformer current will reduce after reaching steady state.

Final analysis that we made is eddy current analysis. We made this analysis to estimate the AC resistance of the windings and to observe the current density in those windings. Current density can be seen in Fig 9.




Figure 9. Current density of a single wire in primary winding.

As expected, we see nonhomogeneous current distribution in the conductor due to skin and proximity effects. More important than to see the current distribution is to get the AC resistance to accurately calculate copper losses in the transformer.





Figure 10. DC and AC resistances of primary winding (mΩ).

As we can see in Fig 10. Frequency has a significant effect on the resistance. Even though we expected such increase, numerical value of the resistance is found by FEA. Therefore, we used this result (1.869Ω) in Ltspice simulations.

# 5. Component Selection

For the component selection part, there are 3 main subtitles, which are the output capacitor selection, controller passive elements selection and the power semiconductor selection for now to complete the simulations. When we begin to develop the PCB schematics and layouts, there will be also connector selection part.

## 5.1 Output Capacitor Selection

The output capacitor should be selected to reduce output voltage ripple while also keeping in view the larger size and price of a larger capacitor. The minimum output capacitor can be calculated using the equation as below:

*where Ilim = Maximum primary current = 100mV/Rsense*

In this equation, we found the minimum output capacitor value. However, we chose 470 capacitor for better filtering and to minimize the EMI effect.

Xxxxxxxxx ESR xxxxxxxx MATERIAL

## 5.2 Controller Passive Elements Selection

### 5.2.1 Snubber Resistance Selection

The proposed design solution for the RC snubber is to power up at low voltage to prevent overvoltage stress, calculate the duration of the ringing on the MOSFET's drain when the power switch turns off without the snubber, and then apply capacitance CSnubber until the ringing period is 1.5 to 2 times longer. To find the snubber resistance, we first need to find leakage inductance. The leakage inductance depends on the coupling coefficient. Coupling coefficients of k=99 percent are typical, and they are determined by the transformer's structure and materials.

Now, we can find the snubber resistance with equation below. The capacitor value here is taken from the datasheet of the mosfet we have chose.

### 5.2.2 Feedback Resistances Selection

The isolated output voltage is controlled by the LT8316 using a special sampling scheme. The scheme experiences repeatable delays and error sources due to its sampling design, which would influence the output voltage and cause a reevaluation of the resistor values. So, the controller needs feedback resistors to regulate this situation. According to the datasheet, in order to determine the values of these resistors, we need to assign a value to one of them and find the other with the equation below.

### 5.2.3 RIREG/SS Selection

This resistor is used to regulate the output current. We can find the resistance value we need to use with the equation given below:

According to the above equation, we found the required resistance value of 68.9kΩ

### 5.2.4 Sense Resistor Selection

We need a sense resistor to be able to set the maximum current. In the datasheet of the controller we chose, the formula for Rsense is shown as below:

### 5.2.5 Boundary Mode Detection Capacitor

Application note of the controller suggest to use 47pF capacitor and check if the operating point is in boundary condition. If not, it is suggested to increase this capacitor up to 100pF. 47pF was satisfactory for our application so we selected this value.

### 5.2.6 Additional Component

CDRV, CBIAS and Vc capacitors are not specified as application dependent capacitors in the datasheet. Therefore, we used same values capacitors as given in the typical application.

Bias diode is also not specified in the application note but it is denoted with fast diode symbol. We will choose this diode according to the simulation results.

## 5.3 Semiconductor Selection

### 5.3.1 Snubber Diodes Selection

**Fast recovery**: According to the application note, breakdown voltage of this diode must be greater than the drain pin voltage of the MOSFET.

XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXX

**Zener:** Zener voltage must be largest possible value withing given limitations. And it is recommended to use around 500 mV Zener diode in the snubber. According to the controller's datasheet, we can calculate the maximum voltage capacity of the Zener diode with the following equation:

XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXX

### 5.3.2 MOSFET Selection

As can be seen from the simulation result in Figures 11 and 12, the maximum voltage is around 450V and current value is around 3.6A on the MOSFET. While choosing the MOSFET, we made a choice considering these values.




Figure 11. MOSFET voltage graph.




Figure 12. MOSFET current graph.

### 5.3.3 Output Diode Selection

The Figures below, namely Figure 13 and Figure 14, show the reverse voltage of the diode and the peak forward current. According to these graphs, the reverse voltage on the diode is around 65. The current flowing on it is approximately 35 A. We should choose the output diode by considering these criteria.




Figure 13. Output diode voltage graph.




Figure 14. Output diode current graph.

# 6. LTspice Simulation Results

We divided LTspice simulation results into three subtitles, which are Steady-State Full-Load Responses, Load Regulation and Line Regulation. To do that, we constructed all the circuit on the LTspice by reducing the ideality of the circuit by adding some of the real-time application parameters such as Leakage inductances and series resistance of the primary and secondary side of the transformer. The overall simulation model is given in the Fig.15.




Figure 15. Project design schematic.

## 6.1 Steady-State Full-Load Responses




Figure 16. Output Voltage at 400 V input.




Figure 17. Output Voltage at 220 V input.

From the steady-state full load analysis of the converter at 400 V maximum input and 220 V minimum input conditions, which are given in the Fig.16 and Fig. 17 respectively, we can claim that the output voltage of the controller is including ripple less than %4. As a proof,

## 6.2 Load Regulation




Figure 18. Light Load to Full Load Response.




Figure 19. Full Load to Light Load Response.

The load regulation simulations were conducted as two part, which are heavy load to light load and vice versa. The results are given in Fig. 18 and Fig. 19. From the figures, we can say that the results are satisfying the load regulation limitation. As a proof,

## 6.3 Line Regulation




Figure 20. 220V to 400V Response.




Figure 21. 400V to 220V Response.

The line regulation simulations were conducted as two part, which are 220 V input to 400V and vice versa. The results are given in Fig. 20 and Fig. 21. From the figures, we can say that the results are satisfying the line regulation limitation. As a proof,

# 7. Conclusion

# 8. References

1. Topology Key to Power Density in Isolated DC-DC Converters. (n.d.). Retrieved April 27, 2021, from <https://www.powerelectronics.com/technologies/dc-dc-converters/article/21854364/topology-key-to-power-density-in-isolated-dcdc-converters>